{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Report","Inverter Data","Panel Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":24,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Report","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,0,0,5],[22,0,25,5],[12,1,12,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[6,1,6,5],[7,1,7,5],[8,1,8,5],[9,1,9,5],[10,1,10,5],[11,0,11,5],[1,1,1,3]]}
["Inverter Sizing Report\nVersion 9.3"]
["Module Model",null,null,null,{"$f":"TODAY()","v":"2021-06-09"},{"$f":"NOW()","v":44356.647048726853}]
["Module Size (W)"]
["Inverter model"]
["AC Rating (kW)"]
[]
["Total Panels"]
["DC Power (kWDC)"]
["DC:AC Ratio"]
["MAX DC Voltage (V)"]
["MAX DC Current (A Total)"]
[]
["Modules per MPPT"]
["MPPT 1",null,"MPPT 7",null,"MPPT 13"]
["MPPT 2",null,"MPPT 8",null,"MPPT 14"]
["MPPT 3",null,"MPPT 9"]
["MPPT 4",null,"MPPT 10"]
["MPPT 5",null,"MPPT 11"]
["MPPT 6",null,"MPPT 12"]
[]
["Lowest Tempeature",null,"Albedo"]
["Highest Temperature"]
["Canadian Solar Inc. (CSI) reserves the right to make any adjustments to the information described herein without notice.  This string sizing tool and the associated report are for general guidance only and, as such, CSI shall not be held responsible for any errors in system design related to this tool.  It is the responsibility of the installer and system designer to ensure that each system is designed to meet all local codes and safety requirements."]

{"sheet":"Inverter Data","index":1,"n_rows":54,"n_cols":12,"rows_kept":54,"cut":false,"hidden":false,"merged":[]}
["Model Number","AC Rating","Max DC ipnut","Max Input per MPPT","Max Input Current","Short Circuit Current","Max DC Voltage","Start Voltage","Strings per MPPT","MPPT","DC:AC","NOM"]
["UL Inverters"]
["CSI-25KTL-GS-FLB",25000,37500,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-30KTL-GS-FLB",30000,45000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-36KTL-GS-FLB",36000,54000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-40KTL-GS-FLB",40000,54000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-50KTL-GS-FLB",50000,64000,16000,22,55,1000,200,4,4,1.75,1.5]
["CSI-40KTL-GS-B",40000,54000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-25K-T480GL01-UB",25000,37500,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-30K-T480GL01-UB",30000,45000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-36K-T480GL01-UB",36000,54000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-40K-T480GL01-UB",40000,54000,13500,18,28.1,1000,350,2,4,1.75,1.5]
["CSI-50KTL-GS-B",50000,75000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-60KTL-GS-B",60000,90000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-66KTL-GS-B",66000,90000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-50K-T480GL01-UB",50000,75000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-60K-T480GL01-UB",60000,90000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-66K-T480GL01-UB",66000,90000,22500,28.5,55,1000,200,4,4,1.75,1.5]
["CSI-75K-T500GL02-U",75000,112500,18750,26,40,1000,195,2,8,2,1.5]
["CSI-100K-T500GL02-U",100000,150000,18750,26,40,1000,195,2,10,2,1.5]
["CSI-125K-T600GL02-U",125000,187500,187500,150,300,1500,900,1,1,1.75,1.5]
["CSI-125KTL-GS-E",125000,187500,187500,150,300,1500,900,20,1,1.75,1.5]
["CSI-255K-T800GL02-U",255000,382500,382500,26,40,1500,620,2,14,2,1.5]
["IEC Inverters"]
["CSI-7KTL1P-GI-FL",7000,8000,4000,10,15.6,600,120,1,3,1.5,1.2]
["CSI-8KTL1P-GI-FL",8000,9200,4000,10,15.6,600,120,1,3,1.5,1.2]
["CSI-9KTL1P-GI-FL",9000,10800,4000,10,15.6,600,120,1,3,1.5,1.2]
["CSI-15KTL-GI-LFL",15000,18000,13500,20,28.1,1000,350,2,2,1.5,1.2]
["CSI-20KTL-GI-LFL",20000,24000,13500,20,28.1,1000,350,2,2,1.5,1.2]
["CSI-20KTL-GI-FL",20000,23000,13500,18,28.1,1000,350,2,4,1.5,1.2]
["CSI-25KTL-GI-FL",25000,28000,13500,18,28.1,1000,350,2,4,1.5,1.2]
["CSI-30KTL-GI-FL",30000,34000,13500,18,28.1,1000,350,2,4,1.5,1.2]
["CSI-30KTL-GI-L",30000,36000,16000,28.5,44.5,1100,200,3,2,1.5,1.2]
["CSI-40KTL-GI-HFL",40000,45000,13500,18,28.1,1000,350,2,4,1.5,1.2]
["CSI-40KTL-GI-FL",40000,48000,16000,22,34.299999999999997,1000,200,2,4,1.5,1.2]
["CSI-50KTL-GI",50000,60000,16000,22,34.299999999999997,1000,200,2,4,1.5,1.2]
["CSI-50KTL-GI-HFL",50000,58000,22500,28.5,44.5,1000,200,3,4,1.5,1.2]
["CSI-60KTL-GI-H",60000,72000,22500,28.5,44.5,1000,200,3,4,1.5,1.2]
["CSI-25K-T400GL02-E",25000,33000,18750,26,40,1100,180,2,3,1.5,1.32]
["CSI-30K-T400GL02-E",30000,39000,18750,26,40,1100,180,2,3,1.5,1.3]
["CSI-33K-T400GL02-E",33000,43000,18750,26,40,1100,180,2,3,1.5,1.3]
["CSI-36K-T400GL02-E",36000,47000,18750,26,40,1100,180,2,4,1.5,1.3]
["CSI-40K-T400GL02-E",40000,52000,18750,26,40,1100,180,2,4,1.5,1.3]
["CSI-40K-T500GL02-E",40000,52000,18750,26,40,1100,180,2,4,1.5,1.3]
["CSI-50K-T400GL02-E",50000,65000,18750,26,40,1100,180,2,4,1.5,1.3]
["CSI-80K-T400GL02-E",80000,104000,18750,26,40,1100,195,2,9,1.5,1.3]
["CSI-100K-T400GL02-E",100000,130000,18750,26,40,1100,195,2,10,1.5,1.3]
["CSI-110K-T400GL02-E",110000,143000,18750,26,40,1100,195,2,10,1.5,1.3]
["CSI-80K-T400GL02-ZA",80000,104000,18750,26,40,1100,195,2,9,1.5,1.3]
["CSI-100K-T400GL02-ZA",100000,130000,18750,26,40,1100,195,2,10,1.5,1.3]
["CSI-110K-T400GL02-ZA",110000,143000,18750,26,40,1100,195,2,10,1.5,1.3]
["CSI-125KTL-GI-E",125000,187500,187500,150,300,1500,900,20,1,1.5,1.5]
["CSI-125K-T600GL02-E",125000,187500,187500,150,300,1500,900,20,1,1.5,1.5]
["CSI-255K-T800GL02-E",255000,382500,382500,26,40,1500,620,2,14,1.75,1.5]

{"sheet":"Panel Data","index":2,"n_rows":199,"n_cols":10,"rows_kept":199,"cut":false,"hidden":false,"merged":[]}
["Model","Cell type ","Rated power @ STC (W) ","Max. power voltage (Vmp)","Max. power current (Imp)","Open-circuit voltage (Voc)","Short-circuit current (Isc)","Pmp temp. coefficient (%/°C)","Voc temp. coefficient (%/°C)","Series fuse rating (A)"]
["CS1H-320MS","MONO",320,36.200000000000003,8.85,44,9.41,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS1H-325MS","MONO",325,36.6,8.8800000000000008,44.1,9.4499999999999993,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS1H-330MS","MONO",330,37,8.92,44.2,9.49,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS1H-335MS","MONO",335,37.4,8.9600000000000009,44.3,9.5299999999999994,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS1H-340MS","MONO",340,37.799999999999997,9,44.5,9.57,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS1H-345MS","MONO",345,38.200000000000003,9.0399999999999991,44.6,9.61,-3.7000000000000002E-3,-2.8999999999999998E-3,15]
["CS3K-300MS","MONO",300,32.5,9.24,39.299999999999997,9.82,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-305MS","MONO",305,32.700000000000003,9.33,39.5,9.9,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-310MS","MONO",310,32.9,9.43,39.700000000000003,9.98,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-315MS","MONO",315,33.1,9.52,39.9,10.06,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-320MS","MONO",320,33.299999999999997,9.61,40.1,10.14,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-325MS","MONO",325,33.5,9.7100000000000009,40.299999999999997,10.220000000000001,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-330MS","MONO",330,33.700000000000003,9.8000000000000007,40.5,10.3,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-335MS","MONO",335,33.9,9.89,41.2,10.39,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3K-285P HE","POLY",285,32.1,8.92,38.700000000000003,9.42,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-290P HE","POLY",290,32.299999999999997,8.98,38.9,9.49,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-295P HE","POLY",295,32.5,9.08,39.1,9.57,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-300P HE","POLY",300,32.700000000000003,9.18,39.299999999999997,9.65,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-315P HE","POLY",315,33.299999999999997,9.4600000000000009,39.9,9.89,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-320P HE","POLY",320,33.5,9.56,40.1,9.9700000000000006,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-325P HE","POLY",325,33.700000000000003,9.65,40.9,10.210000000000001,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-330P HE","POLY",330,33.9,9.74,41.1,10.29,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3K-305P HE","POLY",305,32.9,9.2799999999999994,39.5,9.73,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3L-325P","POLY",325,32,10.16,39,10.74,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-330P","POLY",330,32.200000000000003,10.24,39.200000000000003,10.82,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-335P","POLY",335,32.4,10.34,39.4,10.9,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-340P","POLY",340,32.6,10.43,39.6,10.98,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-345P","POLY",345,32.799999999999997,10.52,39.799999999999997,11.06,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-350P","POLY",350,33,10.61,40.200000000000003,11.24,-3.5999999999999999E-3,-2.8E-3,20]
["CS3L-350MS","MONO",350,33.299999999999997,10.52,40,11.28,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-355MS","MONO",355,33.5,10.61,40.200000000000003,11.33,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-360MS","MONO",360,33.700000000000003,10.69,40.4,11.4,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-365MS","MONO",365,33.9,10.78,40.6,11.47,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-370MS","MONO",370,34.1,10.86,40.799999999999997,11.54,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-375MS","MONO",375,34.299999999999997,10.94,41,11.61,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3L-380MS","MONO",380,34.5,11.02,41.2,11.68,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-400MS","MONO",400,37.200000000000003,10.76,44.5,11.5,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-405MS","MONO",405,37.4,10.83,44.7,11.56,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-410MS","MONO",410,37.6,10.92,44.9,11.62,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-415MS","MONO",415,37.799999999999997,10.98,45.1,11.68,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-420MS","MONO",420,38,11.06,45.3,11.74,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3N-425MS","MONO",425,38.200000000000003,11.13,45.5,11.8,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS1Y-390MS","MONO",390,43.1,9.0500000000000007,51.9,9.82,-3.7000000000000002E-3,-2.8999999999999998E-3,16]
["CS1Y-395MS","MONO",395,43.3,9.1300000000000008,52.1,9.86,-3.7000000000000002E-3,-2.8999999999999998E-3,16]
["CS1Y-400MS","MONO",400,43.5,9.1999999999999993,52.3,9.9,-3.7000000000000002E-3,-2.8999999999999998E-3,16]
["CS1Y-405MS","MONO",405,43.7,9.27,52.5,9.94,-3.7000000000000002E-3,-2.8999999999999998E-3,16]
["CS3U-355MS","MONO",355,39,9.11,46.8,9.61,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-360MS","MONO",360,39.200000000000003,9.19,47,9.69,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-365MS","MONO",365,39.4,9.27,47.2,9.77,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-370MS","MONO",370,39.6,9.35,47.4,9.85,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-375MS","MONO",375,39.799999999999997,9.43,47.6,9.93,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-380MS","MONO",380,40,9.5,47.8,10.01,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-385MS","MONO",385,40.200000000000003,9.58,48,10.09,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-390MS","MONO",390,40.4,9.66,48.2,10.17,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-395MS","MONO",395,40.6,9.73,48.4,10.25,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-400MS","MONO",400,40.799999999999997,9.81,48.6,10.33,-3.5999999999999999E-3,-2.8999999999999998E-3,30]
["CS3U-360MB-AG","MONO BIFACIAL",360,39.200000000000003,9.19,47,9.69,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-365MB-AG","MONO BIFACIAL",365,39.4,9.27,47.2,9.77,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-370MB-AG","MONO BIFACIAL",370,39.6,9.35,47.4,9.85,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-375MB-AG","MONO BIFACIAL",375,39.799999999999997,9.43,47.6,9.93,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-380MB-AG","MONO BIFACIAL",380,40,9.5,47.8,10.01,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-385MB-AG","MONO BIFACIAL",385,40.200000000000003,9.58,48,10.09,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-390MB-AG","MONO BIFACIAL",390,40.4,9.66,48.2,10.17,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-395MB-AG","MONO BIFACIAL",395,40.6,9.73,48.4,10.25,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-400MB-AG","MONO BIFACIAL",400,40.799999999999997,9.81,48.6,10.33,-3.5999999999999999E-3,-2.8999999999999998E-3,25]
["CS3U-345P HE","POLY",345,39,8.86,46.4,9.43,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-350P HE","POLY",350,39.200000000000003,8.94,46.6,9.51,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-355P HE","POLY",355,39.4,9.02,46.8,9.59,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-360P HE","POLY",360,39.6,9.1,47,9.67,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-365P HE","POLY",365,39.799999999999997,9.18,47.2,9.75,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-370P HE","POLY",370,40,9.26,47.4,9.83,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-375P SE","POLY",375,40.200000000000003,9.34,47.6,9.91,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-380P SE","POLY",380,40.4,9.42,47.8,9.99,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-385P SE","POLY",385,40.6,9.5,48,10.07,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-390P SE","POLY",390,40.799999999999997,9.56,48.6,10.17,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-395P SE","POLY",395,41,9.64,48.8,10.24,-3.7000000000000002E-3,-2.8999999999999998E-3,30]
["CS3U-350PB-AG","POLY BIFACIAL",350,39.200000000000003,8.94,46.6,9.51,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-355PB-AG","POLY BIFACIAL",355,39.4,9.02,46.8,9.59,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-360PB-AG","POLY BIFACIAL",360,39.6,9.1,47,9.67,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-365PB-AG","POLY BIFACIAL",365,39.799999999999997,9.18,47.2,9.75,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-370PB-AG","POLY BIFACIAL",370,40,9.26,47.4,9.83,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-375PB-AG","POLY BIFACIAL",375,40.200000000000003,9.34,47.6,9.91,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3U-380PB-AG","POLY BIFACIAL",380,40.4,9.42,47.8,9.99,-3.7000000000000002E-3,-2.8999999999999998E-3,25]
["CS3W-395P HE","POLY",395,38.5,10.26,47,10.82,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-400P HE","POLY",400,38.700000000000003,10.34,47.2,10.9,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-405P HE","POLY",405,38.9,10.42,47.4,10.98,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-410P HE","POLY",410,39.1,10.49,47.6,11.06,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-415P HE","POLY",415,39.299999999999997,10.56,47.8,11.14,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-420P HE","POLY",420,39.5,10.64,48,11.26,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-425P HE","POLY",425,39.700000000000003,10.71,48.2,11.29,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-430P SE","POLY",430,39.9,10.78,48.4,11.32,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-435P SE","POLY",435,40.1,10.85,48.6,11.35,-3.5999999999999999E-3,-2.8E-3,20]
["CS3W-425MS","MONO",425,39.5,10.76,47.7,11.37,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-430MS","MONO",430,39.700000000000003,10.84,47.9,11.42,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-435MS","MONO",435,40.5,10.75,48.5,11.42,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-440MS","MONO",440,40.700000000000003,10.82,48.7,11.48,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-445MS","MONO",445,40.9,10.89,48.9,11.54,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-450MS","MONO",450,41.1,10.96,49.1,11.6,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-455MS","MONO",455,41.3,11.02,49.3,11.66,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-460MS","MONO",460,41.5,11.09,49.5,11.72,-3.5000000000000001E-3,-2.7000000000000001E-3,20]
["CS3W-390PB-AG HE","POLY BIFACIAL",390,38.299999999999997,10.19,46.8,10.74,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-395PB-AG HE","POLY BIFACIAL",395,38.5,10.26,47,10.82,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-400PB-AG HE","POLY BIFACIAL",400,38.700000000000003,10.34,47.2,10.9,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-405PB-AG HE","POLY BIFACIAL",405,38.9,10.42,47.4,10.98,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-410PB-AG HE","POLY BIFACIAL",410,39.1,10.49,47.6,11.06,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-415PB-AG HE","POLY BIFACIAL",415,39.299999999999997,10.56,47.8,11.14,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-420PB-AG SE","POLY BIFACIAL",420,39.5,10.64,48,11.26,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-425PB-AG SE","POLY BIFACIAL",425,39.700000000000003,10.71,48.2,11.29,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-430PB-AG SE","POLY BIFACIAL",430,39.9,10.78,48.4,11.32,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-435PB-AG SE","POLY BIFACIAL",435,40.1,10.85,48.6,11.35,-3.5999999999999999E-3,-2.8E-3,25]
["CS3W-420MB-AG","MONO BIFACIAL",420,39.299999999999997,10.69,47.5,11.33,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-425MB-AG","MONO BIFACIAL",425,39.5,10.76,47.7,11.37,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-430MB-AG","MONO BIFACIAL",430,40.299999999999997,10.68,48.3,11.37,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-435MB-AG","MONO BIFACIAL",435,40.5,10.75,48.5,11.42,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-440MB-AG","MONO BIFACIAL",440,40.700000000000003,10.82,48.7,11.48,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-445MB-AG","MONO BIFACIAL",445,40.9,10.89,48.9,11.54,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-450MB-AG","MONO BIFACIAL",450,41.1,10.96,49.1,11.6,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3W-455MB-AG","MONO BIFACIAL",455,41.3,11.02,49.3,11.66,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS3Y-435P HE","POLY",435,41.8,10.41,51,11.13,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-440P HE","POLY",440,42,10.48,51.2,11.18,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-445P HE","POLY",445,42.2,10.55,51.4,11.23,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-450P HE","POLY",450,42.4,10.62,51.6,11.28,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-455P HE","POLY",455,42.6,10.69,51.8,11.33,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-460P HE","POLY",460,42.8,10.75,52,11.38,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-465P SE","POLY",465,43,10.82,52.2,11.43,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-470P SE","POLY",470,43.2,10.88,52.4,11.48,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-475P SE","POLY",475,43.4,10.95,52.6,11.53,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-480P SE","POLY",480,43.6,11.01,52.8,11.58,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-485P SE","POLY",485,43.8,11.08,53,11.63,-3.5999999999999999E-3,-2.8E-3,20]
["CS3Y-475MS","MONO",475,44,10.81,52.7,11.52,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-480MS","MONO",480,44.2,10.87,52.9,11.57,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-485MS","MONO",485,44.4,10.94,53.1,11.62,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-490MS","MONO",490,44.6,11,53.3,11.67,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-495MS","MONO",495,44.8,11.06,53.5,11.72,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-500MS","MONO",500,45,11.12,53.7,11.77,-3.3999999999999998E-3,-2.5999999999999999E-3,20]
["CS3Y-430PB-AG HE","POLY BIFACIAL",430,41.6,10.34,50.8,10.98,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-435PB-AG HE","POLY BIFACIAL",435,41.8,10.41,51,11.03,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-440PB-AG HE","POLY BIFACIAL",440,42,10.48,51.2,11.08,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-445PB-AG HE","POLY BIFACIAL",445,42.2,10.55,51.4,11.13,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-450PB-AG HE","POLY BIFACIAL",450,42.4,10.62,51.6,11.18,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-455PB-AG HE","POLY BIFACIAL",455,42.6,10.69,51.8,11.33,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-460PB-AG SE","POLY BIFACIAL",460,42.8,10.75,52,11.38,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-465PB-AG SE","POLY BIFACIAL",465,43,10.82,52.2,11.43,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-470PB-AG SE","POLY BIFACIAL",470,43.2,10.88,52.4,11.48,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-475PB-AG SE","POLY BIFACIAL",475,43.4,10.95,52.6,11.53,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-480PB-AG SE","POLY BIFACIAL",480,43.6,11.01,52.8,11.58,-3.5999999999999999E-3,-2.8E-3,25]
["CS3Y-465MB-AG","MONO BIFACIAL",465,43.6,10.67,52.3,11.42,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS3Y-470MB-AG","MONO BIFACIAL",470,43.8,10.74,52.5,11.47,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS3Y-475MB-AG","MONO BIFACIAL",475,44,10.81,52.7,11.52,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS3Y-480MB-AG","MONO BIFACIAL",480,44.2,10.87,52.9,11.57,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS3Y-485MB-AG","MONO BIFACIAL",485,44.4,10.94,53.1,11.62,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS3Y-490MB-AG","MONO BIFACIAL",490,44.6,11,53.3,11.67,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-525MS","MONO",525,40.700000000000003,12.9,48.6,13.75,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-530MS","MONO",530,40.9,12.96,48.8,13.8,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-535MS","MONO",535,41.1,13.02,49,13.85,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-540MS","MONO",540,41.3,13.08,49.2,13.9,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-545MS","MONO",545,41.5,13.14,49.4,13.95,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-550MS","MONO",550,41.7,13.2,49.6,14,-3.3999999999999998E-3,-2.5999999999999999E-3,25]
["CS6W-520MB-AG","MONO BIFACIAL",520,40.5,12.84,48.4,13.7,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6W-525MB-AG","MONO BIFACIAL",525,40.700000000000003,12.9,48.6,13.75,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6W-530MB-AG","MONO BIFACIAL",530,40.9,12.96,48.8,13.8,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6W-535MB-AG","MONO BIFACIAL",535,41.1,13.02,49,13.85,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6W-540MB-AG","MONO BIFACIAL",540,41.3,13.08,49.2,13.9,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6W-545MB-AG","MONO BIFACIAL",545,41.5,13.14,49.4,13.95,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS6Y-570MS","MONO",570,43.8,13.02,52.8,13.77,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS6Y-575MS","MONO",575,44,13.07,53,13.82,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS6Y-580MS","MONO",580,44.2,13.13,53.2,13.87,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS6Y-585MS","MONO",585,44.4,13.18,53.4,13.92,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS6Y-590MS","MONO",590,44.6,13.23,53.6,13.97,-3.5000000000000001E-3,-2.7000000000000001E-3,25]
["CS6Y-565MB-AG","MONO BIFACIAL",565,43.6,12.96,52.6,13.72,-3.5000000000000001E-3,-2.7000000000000001E-3,30]
["CS6Y-570MB-AG","MONO BIFACIAL",570,43.8,13.02,52.8,13.77,-3.5000000000000001E-3,-2.7000000000000001E-3,30]
["CS6Y-575MB-AG","MONO BIFACIAL",575,44,13.07,53,13.82,-3.5000000000000001E-3,-2.7000000000000001E-3,30]
["CS6Y-580MB-AG","MONO BIFACIAL",580,44.2,13.13,53.2,13.87,-3.5000000000000001E-3,-2.7000000000000001E-3,30]
["CS6Y-585MB-AG","MONO BIFACIAL",585,44.4,13.18,53.4,13.92,-3.5000000000000001E-3,-2.7000000000000001E-3,30]
["CS7L-580MS","MONO",580,34.1,17.02,40.5,18.27,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-585MS","MONO",585,34.299999999999997,17.059999999999999,40.700000000000003,18.32,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-590MS","MONO",590,34.5,17.11,40.9,18.37,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-595MS","MONO",595,34.700000000000003,17.149999999999999,41.1,18.420000000000002,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-600MS","MONO",600,34.9,17.2,41.3,18.47,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-605MS","MONO",605,35.1,17.25,41.5,18.52,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7L-570MB-AG","MONO BIFACIAL",570,33.700000000000003,16.93,40.1,18.170000000000002,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-575MB-AG","MONO BIFACIAL",575,33.9,16.97,40.299999999999997,18.22,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-580MB-AG","MONO BIFACIAL",580,34.1,17.02,40.5,18.27,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-585MB-AG","MONO BIFACIAL",585,34.299999999999997,17.059999999999999,40.700000000000003,18.32,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-590MB-AG","MONO BIFACIAL",590,34.5,17.11,40.9,18.37,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-595MB-AG","MONO BIFACIAL",595,34.700000000000003,17.149999999999999,41.1,18.420000000000002,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7L-600MB-AG","MONO BIFACIAL",600,34.9,17.2,41.3,18.47,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7N-640MS","MONO",640,37.5,17.07,44.6,18.309999999999999,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-645MS","MONO",645,37.700000000000003,17.11,44.8,18.350000000000001,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-650MS","MONO",650,37.9,17.16,45,18.39,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-655MS","MONO",655,38.1,17.2,45.2,18.43,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-660MS","MONO",660,38.299999999999997,17.239999999999998,45.4,18.47,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-665MS","MONO",665,38.5,17.28,45.6,18.510000000000002,-3.3999999999999998E-3,-2.5999999999999999E-3,30]
["CS7N-635MB-AG","MONO BIFACIAL",635,37.299999999999997,17.03,44.4,18.27,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7N-640MB-AG","MONO BIFACIAL",640,37.5,17.07,44.6,18.309999999999999,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7N-645MB-AG","MONO BIFACIAL",645,37.700000000000003,17.11,44.8,18.350000000000001,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7N-650MB-AG","MONO BIFACIAL",650,37.9,17.16,45,18.39,-3.3999999999999998E-3,-2.5999999999999999E-3,35]
["CS7N-655MB-AG","MONO BIFACIAL",655,38.1,17.2,45.2,18.43,-3.3999999999999998E-3,-2.5999999999999999E-3,35]